CGAL 6.1.1 - Triangulated Surface Mesh Deformation

Loading...
Searching...
No Matches
List of all members
CGAL::Surface_mesh_deformation< TM, VIM, HIM, TAG, WC, ST, CR, VPM > Class Template Reference
Reference Manual

`#include <CGAL/Surface_mesh_deformation.h>`

## Definition

template<class TM, class VIM = Default, class HIM = Default, Deformation_algorithm_tag TAG = SPOKES_AND_RIMS, class WC = Default, class ST = Default, class CR = Default, class VPM = Default>
class CGAL::Surface_mesh_deformation< TM, VIM, HIM, TAG, WC, ST, CR, VPM >

Class providing the functionalities for deforming a triangulated surface mesh.

Template Parameters

  TM | a model of `HalfedgeGraph`
  VIM | a model of `ReadablePropertyMap` with `Surface_mesh_deformation::vertex_descriptor` as key and `unsigned int` as value type. The default is `boost::property_map<TM, boost::vertex_index_t>::type`.
  HIM | a model of `ReadablePropertyMap` with `Surface_mesh_deformation::halfedge_descriptor` as key and `unsigned int` as value type. The default is `boost::property_map<TM, boost::halfedge_index_t>::type`.
  TAG | tag for selecting the deformation algorithm
  WC | a model of SurfaceMeshDeformationWeights, with `WC::Triangle_mesh` being `TM`. If `TAG` is `ORIGINAL_ARAP`, the weights must be positive to guarantee a correct energy minimization. The default is the cotangent weighting scheme. In case `TAG` is `ORIGINAL_ARAP`, negative weights are clamped to zero.
  ST | a model of SparseLinearAlgebraWithFactorTraits_d. If Eigen 3.2 (or greater) is available and `CGAL_EIGEN3_ENABLED` is defined, then an overload of `Eigen_solver_traits` is provided as default parameter. CGAL::Eigen_solver_traits< Eigen::SparseLU< CGAL::Eigen_sparse_matrix<double>::EigenType, Eigen::COLAMDOrdering<int> > > CGAL::Eigen_solver_traits CGAL::Eigen_sparse_matrix::EigenType Eigen::SparseMatrix< T > EigenType
  CR | a model of DeformationClosestRotationTraits_3. If Eigen 3.1 (or greater) is available and `CGAL_EIGEN3_ENABLED` is defined, `Deformation_Eigen_polar_closest_rotation_traits_3` is provided as default parameter.
  VPM | a model of `ReadWritePropertyMap` with `Surface_mesh_deformation::vertex_descriptor` as key and a point as value type. The point type must be a model of `RawPoint_3`. The default is `boost::property_map<TM, CGAL::vertex_point_t>::type`.

Examples
  Surface_mesh_deformation/all_roi_assign_example.cpp, Surface_mesh_deformation/custom_weight_for_edges_example.cpp, Surface_mesh_deformation/deform_mesh_for_botsch08_format_sre_arap.cpp, Surface_mesh_deformation/deform_polyhedron_with_custom_pmap_example.cpp, and Surface_mesh_deformation/k_ring_roi_translate_rotate_example.cpp.

## Types
typedef TM | Triangle_mesh
| Triangle mesh type.
typedef VIM | Vertex_index_map
| vertex index map type
typedef HIM | Hedge_index_map
| halfedge index map type
typedef ST | Sparse_linear_solver
| sparse linear solver type
typedef CR | Closest_rotation_traits
| closest rotation traits type
typedef VPM | Vertex_point_map
| vertex point map type
typedef WC | Weight_calculator
| weight calculator functor type
typedef boost::graph_traits< Triangle_mesh >::vertex_descriptor | vertex_descriptor
| The type for vertex descriptor.
typedef boost::graph_traits< Triangle_mesh >::halfedge_descriptor | halfedge_descriptor
| The type for halfedge descriptor.
typedef boost::property_traits< Vertex_point_map >::value_type | Point
| The 3D point type, model of `RawPoint_3`
typedef std::vector< vertex_descriptor > | Roi_vertex_range
| A constant iterator range over the vertices of the region-of-interest.

## Construction
| Surface_mesh_deformation (Triangle_mesh &triangle_mesh, Vertex_index_map vertex_index_map=unspecified_internal_vertex_index_map, Hedge_index_map hedge_index_map=unspecified_internal_halfedge_index_map, Vertex_point_map vertex_point_map=get(boost::vertex_point, triangle_mesh), Weight_calculator weight_calculator=Weight_calculator(triangle_mesh, vertex_point_map))
| The constructor of a deformation object.

## Preprocessing
void | clear_roi_vertices ()
| Erases all the vertices from the region-of-interest (control vertices included).
void | clear_control_vertices ()
| Erases all the vertices from the set of control vertices.
bool | insert_control_vertex (vertex_descriptor vd)
| Inserts a vertex in the set of control vertices.
template<class InputIterator >
void | insert_control_vertices (InputIterator begin, InputIterator end)
| Inserts a range of vertices in the set of control vertices.
bool | erase_control_vertex (vertex_descriptor vd)
| Erases a vertex from the set of control vertices.
template<class InputIterator >
void | insert_roi_vertices (InputIterator begin, InputIterator end)
| Inserts a range of vertices in the region-of-interest.
bool | insert_roi_vertex (vertex_descriptor vd)
| Inserts a vertex in the region-of-interest.
bool | erase_roi_vertex (vertex_descriptor vd)
| Erases a vertex from the region-of-interest and the set of control vertices.
bool | preprocess ()
| Preprocessing function that need to be called each time the region-of-interest or the set of control vertices are changed before calling `deform()`.

## Deformation
void | set_target_position (vertex_descriptor vd, const Point &target_position)
| Sets the target position of a control vertex.
template<class Vect >
void | translate (vertex_descriptor vd, const Vect &t)
| Updates the target position of `vd` by applying a translation of vector `t`.
template<class InputIterator , class Vect >
void | translate (InputIterator begin, InputIterator end, const Vect &t)
| Equivalent to calling the overload taking only one control vertex, for each vertex in the range `[begin,end[`.
template<typename Quaternion , typename Vect >
void | rotate (vertex_descriptor vd, const Vect &to_rotation_center, const Quaternion &quat)
| Updates the target position of `vd` by applying to its last target position a rotation defined by the quaternion `quat`, the center of the rotation being the origin translated by `to_rotation_center` .
template<typename InputIterator , typename Vect , typename Quaternion >
void | rotate (InputIterator begin, InputIterator end, const Vect &to_rotation_center, const Quaternion &quat)
| Equivalent to calling the overload taking only one control vertex, for each vertex in the range `[begin,end[`.
const Point & | target_position (vertex_descriptor vd)
| Returns the target position of a control vertex.
void | deform ()
| Deforms the region-of-interest according to the deformation algorithm, using the target positions of each control vertex set by using `rotate()`, `translate()`, or `set_target_position()`.
void | deform (unsigned int iterations, double tolerance)
| Same as `deform()` but the number of iterations and the tolerance are one-time parameters.
void | reset ()
| Resets the points associated to the vertices of the region-of-interest at their initial positions at time of the functor construction or after the last call to `overwrite_initial_geometry()`.
void | overwrite_initial_geometry ()
| Sets the initial positions of the vertices from the region-of-interest to the current positions.

## Utilities
unsigned int | iterations ()
| Gets the default number of iterations (5) or the value passed to the function `set_iterations()`
double | tolerance ()
| Gets the default tolerance parameter (1e-4) or the value passed to the function `set_tolerance()`
void | set_iterations (unsigned int iterations)
| Sets the maximum number of iterations ran by `deform()`
void | set_tolerance (double tolerance)
| Sets the tolerance of the convergence used in `deform()`.
const Roi_vertex_range & | roi_vertices () const
| Returns the range of vertices in the region-of-interest.
bool | is_roi_vertex (vertex_descriptor vd) const
| Tests whether a vertex is inside the region-of-interest.
bool | is_control_vertex (vertex_descriptor vd) const
| Tests whether a vertex is a control vertex.
const Triangle_mesh & | triangle_mesh () const
| Provides access to the triangle mesh being deformed.
void | set_sre_arap_alpha (double a)
| Sets the alpha coefficient that determines the weight of the bending term (rotation smoothness) for the SRE-ARAP deformation technique.

## Member Typedef Documentation

## ◆ Roi_vertex_range

template<class TM , class VIM = Default, class HIM = Default, Deformation_algorithm_tag TAG = SPOKES_AND_RIMS, class WC = Default, class ST = Default, class CR = Default, class VPM = Default>

typedef std::vector<vertex_descriptor> CGAL::Surface_mesh_deformation< TM, VIM, HIM, TAG, WC, ST, CR, VPM >::Roi_vertex_range

A constant iterator range over the vertices of the region-of-interest.

It is a model of `ConstRange` with `vertex_descriptor` as iterator value type.

## Constructor & Destructor Documentation

## ◆ Surface_mesh_deformation()

template<class TM , class VIM = Default, class HIM = Default, Deformation_algorithm_tag TAG = SPOKES_AND_RIMS, class WC = Default, class ST = Default, class CR = Default, class VPM = Default>

CGAL::Surface_mesh_deformation< TM, VIM, HIM, TAG, WC, ST, CR, VPM >::Surface_mesh_deformation | ( | Triangle_mesh & | triangle_mesh,
|  | Vertex_index_map | vertex_index_map = `unspecified_internal_vertex_index_map`,
|  | Hedge_index_map | hedge_index_map = `unspecified_internal_halfedge_index_map`,
|  | Vertex_point_map | vertex_point_map = `get(boost::vertex_point, triangle_mesh)`,
|  | Weight_calculator | weight_calculator = `Weight_calculator(triangle_mesh, vertex_point_map)`
| ) |  |

The constructor of a deformation object.

Precondition
  `triangle_mesh` consists of only triangular facets

Parameters

  triangle_mesh | triangulated surface mesh to deform
  vertex_index_map | a property map which associates a unique id to each vertex, between `0` to `num_vertices(triangle_mesh)-1`.
  hedge_index_map | property map which associates a unique id to each halfedge, between `0` to `2*num_edges(triangle_mesh)-1`.
  vertex_point_map | property map which associates a point to each vertex of the triangle mesh.
  weight_calculator | function object or pointer for weight calculation

## Member Function Documentation

## ◆ deform() [1/2]

template<class TM , class VIM = Default, class HIM = Default, Deformation_algorithm_tag TAG = SPOKES_AND_RIMS, class WC = Default, class ST = Default, class CR = Default, class VPM = Default>

void CGAL::Surface_mesh_deformation< TM, VIM, HIM, TAG, WC, ST, CR, VPM >::deform | ( |  | ) |

Deforms the region-of-interest according to the deformation algorithm, using the target positions of each control vertex set by using `rotate()`, `translate()`, or `set_target_position()`.

The points associated to each vertex of the input triangle mesh that are inside the region-of-interest are updated.

Note
  Nothing happens if `preprocess()` returns `false`.

See also
  set_iterations(unsigned int iterations), set_tolerance(double tolerance), deform(unsigned int iterations, double tolerance)

## ◆ deform() [2/2]

template<class TM , class VIM = Default, class HIM = Default, Deformation_algorithm_tag TAG = SPOKES_AND_RIMS, class WC = Default, class ST = Default, class CR = Default, class VPM = Default>

void CGAL::Surface_mesh_deformation< TM, VIM, HIM, TAG, WC, ST, CR, VPM >::deform | ( | unsigned int | iterations,
|  | double | tolerance
| ) |  |

Same as `deform()` but the number of iterations and the tolerance are one-time parameters.

Parameters

  iterations | number of iterations for optimization procedure
  tolerance | tolerance of convergence (see explanations set_tolerance(double tolerance))

## ◆ erase_control_vertex()

template<class TM , class VIM = Default, class HIM = Default, Deformation_algorithm_tag TAG = SPOKES_AND_RIMS, class WC = Default, class ST = Default, class CR = Default, class VPM = Default>

bool CGAL::Surface_mesh_deformation< TM, VIM, HIM, TAG, WC, ST, CR, VPM >::erase_control_vertex | ( | vertex_descriptor | vd | ) |

Erases a vertex from the set of control vertices.

Parameters

  vd | the vertex to be erased

Returns
  `true` if `vd` was a control vertex.

## ◆ erase_roi_vertex()

template<class TM , class VIM = Default, class HIM = Default, Deformation_algorithm_tag TAG = SPOKES_AND_RIMS, class WC = Default, class ST = Default, class CR = Default, class VPM = Default>

bool CGAL::Surface_mesh_deformation< TM, VIM, HIM, TAG, WC, ST, CR, VPM >::erase_roi_vertex | ( | vertex_descriptor | vd | ) |

Erases a vertex from the region-of-interest and the set of control vertices.

Note
  At the next call to `preprocess()`, any vertex that is no longer in the region-of-interest will be assigned to its original position (that is the position of the vertex at the time of construction or after the last call to `overwrite_initial_geometry()`).

Parameters

  vd | the vertex to be erased

Returns
  `true` `vd` was a vertex from the region-of-interest.

## ◆ insert_control_vertex()

template<class TM , class VIM = Default, class HIM = Default, Deformation_algorithm_tag TAG = SPOKES_AND_RIMS, class WC = Default, class ST = Default, class CR = Default, class VPM = Default>

bool CGAL::Surface_mesh_deformation< TM, VIM, HIM, TAG, WC, ST, CR, VPM >::insert_control_vertex | ( | vertex_descriptor | vd | ) |

Inserts a vertex in the set of control vertices.

The vertex is also inserted in the region-of-interest if it is not already in it.

Parameters

  vd | the vertex to be inserted

Returns
  `true` if `vd` is not already a control vertex.

## ◆ insert_control_vertices()

template<class TM , class VIM = Default, class HIM = Default, Deformation_algorithm_tag TAG = SPOKES_AND_RIMS, class WC = Default, class ST = Default, class CR = Default, class VPM = Default>
template<class InputIterator >

void CGAL::Surface_mesh_deformation< TM, VIM, HIM, TAG, WC, ST, CR, VPM >::insert_control_vertices | ( | InputIterator | begin,
|  | InputIterator | end
| ) |  |

Inserts a range of vertices in the set of control vertices.

The vertices are also inserted in the region-of-interest if they are not already in it.

Template Parameters

  InputIterator | input iterator type with `vertex_descriptor` as value type

Parameters

  begin | first iterator of the range of vertices
  end | past-the-end iterator of the range of vertices

## ◆ insert_roi_vertex()

template<class TM , class VIM = Default, class HIM = Default, Deformation_algorithm_tag TAG = SPOKES_AND_RIMS, class WC = Default, class ST = Default, class CR = Default, class VPM = Default>

bool CGAL::Surface_mesh_deformation< TM, VIM, HIM, TAG, WC, ST, CR, VPM >::insert_roi_vertex | ( | vertex_descriptor | vd | ) |

Inserts a vertex in the region-of-interest.

Parameters

  vd | the vertex to be inserted

Returns
  `true` if `vd` is not already in the region-of-interest.

## ◆ insert_roi_vertices()

template<class TM , class VIM = Default, class HIM = Default, Deformation_algorithm_tag TAG = SPOKES_AND_RIMS, class WC = Default, class ST = Default, class CR = Default, class VPM = Default>
template<class InputIterator >

void CGAL::Surface_mesh_deformation< TM, VIM, HIM, TAG, WC, ST, CR, VPM >::insert_roi_vertices | ( | InputIterator | begin,
|  | InputIterator | end
| ) |  |

Inserts a range of vertices in the region-of-interest.

Template Parameters

  InputIterator | input iterator with `vertex_descriptor` as value type

Parameters

  begin | first iterator of the range of vertices
  end | past-the-end iterator of the range of vertices

## ◆ is_control_vertex()

template<class TM , class VIM = Default, class HIM = Default, Deformation_algorithm_tag TAG = SPOKES_AND_RIMS, class WC = Default, class ST = Default, class CR = Default, class VPM = Default>

bool CGAL::Surface_mesh_deformation< TM, VIM, HIM, TAG, WC, ST, CR, VPM >::is_control_vertex | ( | vertex_descriptor | vd | ) | const

Tests whether a vertex is a control vertex.

Parameters

  vd | the query vertex

Returns
  `true` if `vd` has been inserted to (and not erased from) the set of control vertices.

## ◆ is_roi_vertex()

template<class TM , class VIM = Default, class HIM = Default, Deformation_algorithm_tag TAG = SPOKES_AND_RIMS, class WC = Default, class ST = Default, class CR = Default, class VPM = Default>

bool CGAL::Surface_mesh_deformation< TM, VIM, HIM, TAG, WC, ST, CR, VPM >::is_roi_vertex | ( | vertex_descriptor | vd | ) | const

Tests whether a vertex is inside the region-of-interest.

Parameters

  vd | the query vertex

Returns
  `true` if `vd` has been inserted to (and not erased from) the region-of-interest.

## ◆ overwrite_initial_geometry()

template<class TM , class VIM = Default, class HIM = Default, Deformation_algorithm_tag TAG = SPOKES_AND_RIMS, class WC = Default, class ST = Default, class CR = Default, class VPM = Default>

void CGAL::Surface_mesh_deformation< TM, VIM, HIM, TAG, WC, ST, CR, VPM >::overwrite_initial_geometry | ( |  | ) |

Sets the initial positions of the vertices from the region-of-interest to the current positions.

Calling this function has the same effect as creating a new deformation object with the current deformed triangle mesh, keeping the region-of-interest and the set of control vertices.

Note
  if the region-of-interest or the set of control vertices have been modified since the last call to `preprocess()`, it will be called prior to the overwrite.

Advanced

This function might have a non-negligible effect on the result. The Laplacian matrix of the free vertices and the optimal rotations are computed using the original positions of the points associated to the vertices. Thus, if a deformed version of the surface mesh is used as reference, the surface mesh properties the algorithm tries to preserve are those of an altered version (which are already degraded).

## ◆ preprocess()

template<class TM , class VIM = Default, class HIM = Default, Deformation_algorithm_tag TAG = SPOKES_AND_RIMS, class WC = Default, class ST = Default, class CR = Default, class VPM = Default>

bool CGAL::Surface_mesh_deformation< TM, VIM, HIM, TAG, WC, ST, CR, VPM >::preprocess | ( |  | ) |

Preprocessing function that need to be called each time the region-of-interest or the set of control vertices are changed before calling `deform()`.

If not already done, `deform()` first calls this function.

Advanced

Collects the vertices not in the region-of-interest that are adjacent to a vertex from the region-of-interest (these vertices are internally considered as fixed control vertices). Then assembles and factorizes the Laplacian matrix used in the function `deform()`.

Note
  A modification of the set of control vertices or the region-of-interest invalidates the preprocessing data.

Returns
  `true` if successful. A common reason for failure is that the system is rank deficient, which happens for example when all the vertices are in the region-of-interest and no control vertices are set, or if the weighting scheme used features too many zero and breaks the connectivity information.

## ◆ reset()

template<class TM , class VIM = Default, class HIM = Default, Deformation_algorithm_tag TAG = SPOKES_AND_RIMS, class WC = Default, class ST = Default, class CR = Default, class VPM = Default>

void CGAL::Surface_mesh_deformation< TM, VIM, HIM, TAG, WC, ST, CR, VPM >::reset | ( |  | ) |

Resets the points associated to the vertices of the region-of-interest at their initial positions at time of the functor construction or after the last call to `overwrite_initial_geometry()`.

Note
  if the region-of-interest or the set of control vertices have been modified since the last call to `preprocess()`, it will be called prior to the reset.

## ◆ rotate() [1/2]

template<class TM , class VIM = Default, class HIM = Default, Deformation_algorithm_tag TAG = SPOKES_AND_RIMS, class WC = Default, class ST = Default, class CR = Default, class VPM = Default>
template<typename InputIterator , typename Vect , typename Quaternion >

void CGAL::Surface_mesh_deformation< TM, VIM, HIM, TAG, WC, ST, CR, VPM >::rotate | ( | InputIterator | begin,
|  | InputIterator | end,
|  | const Vect & | to_rotation_center,
|  | const Quaternion & | quat
| ) |  |

Equivalent to calling the overload taking only one control vertex, for each vertex in the range `[begin,end[`.

Template Parameters

  InputIterator | input iterator type with `vertex_descriptor` as value type
  Quaternion | is a quaternion class with `Vect operator*(Quaternion, Vect)` returning the product of a quaternion with a vector
  Vect | is a 3D vector class, with `Vect(double x,double y, double z)` being a constructor from its Cartesian coordinates and `double Vect::operator[](int i)` with i=0,1 or 2 returning its Cartesian coordinates.

Parameters

  begin | first iterator of the range of vertices
  end | past-the-end iterator of the range of vertices
  to_rotation_center | the vector to translate the origin to the center of the rotation
  quat | quaternion of the rotation

Precondition
  `quad` represents a rotation

## ◆ rotate() [2/2]

template<class TM , class VIM = Default, class HIM = Default, Deformation_algorithm_tag TAG = SPOKES_AND_RIMS, class WC = Default, class ST = Default, class CR = Default, class VPM = Default>
template<typename Quaternion , typename Vect >

void CGAL::Surface_mesh_deformation< TM, VIM, HIM, TAG, WC, ST, CR, VPM >::rotate | ( | vertex_descriptor | vd,
|  | const Vect & | to_rotation_center,
|  | const Quaternion & | quat
| ) |  |

Updates the target position of `vd` by applying to its last target position a rotation defined by the quaternion `quat`, the center of the rotation being the origin translated by `to_rotation_center` .

Template Parameters

  Quaternion | is a quaternion class with `Vect operator*(Quaternion, Vect)` returning the product of a quaternion with a vector
  Vect | is a 3D vector class, with `Vect(double x,double y, double z)` being a constructor from its Cartesian coordinates and `double Vect::operator[](int i)` with i=0,1 or 2 returning its Cartesian coordinates.

Parameters

  vd | a control vertex
  to_rotation_center | the vector to translate the origin to the center of the rotation
  quat | quaternion of the rotation

Precondition
  `is_control_vertex(vd)`
  `quad` represents a rotation

## ◆ set_sre_arap_alpha()

template<class TM , class VIM = Default, class HIM = Default, Deformation_algorithm_tag TAG = SPOKES_AND_RIMS, class WC = Default, class ST = Default, class CR = Default, class VPM = Default>

void CGAL::Surface_mesh_deformation< TM, VIM, HIM, TAG, WC, ST, CR, VPM >::set_sre_arap_alpha | ( | double | a | ) |

Sets the alpha coefficient that determines the weight of the bending term (rotation smoothness) for the SRE-ARAP deformation technique.

The range of values can be from 0 to infinity. When alpha=0, the method reverts to ARAP. When alpha is increased, neighboring rotations become similar to each other, where alpha=infinity results in a global rigid transformation of the ROI. The value of alpha depends on the surface area and shape. Since alpha is not too sensitive, it can be tweaked in most cases by multiplying it by powers of 10. The default value for alpha is 0.02.

## ◆ set_target_position()

template<class TM , class VIM = Default, class HIM = Default, Deformation_algorithm_tag TAG = SPOKES_AND_RIMS, class WC = Default, class ST = Default, class CR = Default, class VPM = Default>

void CGAL::Surface_mesh_deformation< TM, VIM, HIM, TAG, WC, ST, CR, VPM >::set_target_position | ( | vertex_descriptor | vd,
|  | const Point & | target_position
| ) |  |

Sets the target position of a control vertex.

Parameters

  vd | the control vertex the target position is set
  target_position | the new target position

## ◆ set_tolerance()

template<class TM , class VIM = Default, class HIM = Default, Deformation_algorithm_tag TAG = SPOKES_AND_RIMS, class WC = Default, class ST = Default, class CR = Default, class VPM = Default>

void CGAL::Surface_mesh_deformation< TM, VIM, HIM, TAG, WC, ST, CR, VPM >::set_tolerance | ( | double | tolerance | ) |

Sets the tolerance of the convergence used in `deform()`.

If `tolerance==0`, no energy based termination criteria is used (preventing to do the energy computation at each iteration step)

`tolerance >` \(|\mathrm{energy}(m_i) - \mathrm{energy}(m_{i-1})| / \mathrm{energy}(m_i)\) will be used as a termination criterium.

## ◆ target_position()

template<class TM , class VIM = Default, class HIM = Default, Deformation_algorithm_tag TAG = SPOKES_AND_RIMS, class WC = Default, class ST = Default, class CR = Default, class VPM = Default>

const Point & CGAL::Surface_mesh_deformation< TM, VIM, HIM, TAG, WC, ST, CR, VPM >::target_position | ( | vertex_descriptor | vd | ) |

Returns the target position of a control vertex.

Parameters

  vd | a control vertex

Precondition
  `is_control_vertex(vd)`

## ◆ translate() [1/2]

template<class TM , class VIM = Default, class HIM = Default, Deformation_algorithm_tag TAG = SPOKES_AND_RIMS, class WC = Default, class ST = Default, class CR = Default, class VPM = Default>
template<class InputIterator , class Vect >

void CGAL::Surface_mesh_deformation< TM, VIM, HIM, TAG, WC, ST, CR, VPM >::translate | ( | InputIterator | begin,
|  | InputIterator | end,
|  | const Vect & | t
| ) |  |

Equivalent to calling the overload taking only one control vertex, for each vertex in the range `[begin,end[`.

Template Parameters

  InputIterator | input iterator type with `vertex_descriptor` as value type
  Vect | is a 3D vector class, with `Vect(double x,double y, double z)` being a constructor from its Cartesian coordinates and `double Vect::operator[](int i)` with i=0,1 or 2 returning its Cartesian coordinates.

Parameters

  begin | first iterator of the range of vertices
  end | past-the-end iterator of the range of vertices
  t | translation vector

## ◆ translate() [2/2]

template<class TM , class VIM = Default, class HIM = Default, Deformation_algorithm_tag TAG = SPOKES_AND_RIMS, class WC = Default, class ST = Default, class CR = Default, class VPM = Default>
template<class Vect >

void CGAL::Surface_mesh_deformation< TM, VIM, HIM, TAG, WC, ST, CR, VPM >::translate | ( | vertex_descriptor | vd,
|  | const Vect & | t
| ) |  |

Updates the target position of `vd` by applying a translation of vector `t`.

Template Parameters

  Vect | is a 3D vector class, with `Vect(double x,double y, double z)` being a constructor from its Cartesian coordinates and `double Vect::operator[](int i)` with i=0,1 or 2 returning its Cartesian coordinates.

Parameters

  vd | a control vertex
  t | translation vector

Precondition
  `is_control_vertex(vd)`