CGAL 6.2 - 3D Mesh Generation

Loading...
Searching...
No Matches
CGAL::Compact_mesh_cell_base_3< GT, MD, TDS > Class Template Reference
Reference Manual » Mesh Classes

## Definition

template<class GT, class MD, class TDS = void>
class CGAL::Compact_mesh_cell_base_3< GT, MD, TDS >

The class `Compact_mesh_cell_base_3<GT, MD>` is a model of the concept `MeshCellBase_3`.

It is designed to serve as cell base class for the 3D triangulation used in the 3D mesh generation process. It is more compact in memory than `Mesh_cell_base_3`.

Template Parameters

  GT | is the geometric traits class. It has to be a model of the concept `MeshTriangulationTraits_3`.
  MD | provides the types of indices used to identify the faces of the input complex. It has to be a model of the concept `MeshDomain_3`.
  TDS | is the triangulation data structure class to which cells belong. That parameter is only used by the rebind mechanism (see `TriangulationDSCellBase_3::Rebind_TDS`). Users should always use the default parameter value `void`.

Is model of
  `MeshCellBase_3`

See also
  `CGAL::Mesh_complex_3_in_triangulation_3<Tr,CornerIndex,CurveIndex>`
  `CGAL::Mesh_cell_base_3<GT, MD, Cb>`