CGAL 6.2 - Point Set Processing

Loading...
Searching...
No Matches
Point_set_processing_3/orient_scanlines_example.cpp
#include <CGAL/Simple_cartesian.h>
#include <CGAL/Point_set_3/IO/LAS.h>
#include <CGAL/IO/LAS.h>
#include <CGAL/IO/PLY.h>
#include <CGAL/jet_estimate_normals.h>
#include <CGAL/scanline_orient_normals.h>
using Kernel = CGAL::Simple_cartesian<double>;
using Point_3 = Kernel::Point_3;
using Vector_3 = Kernel::Vector_3;
using Point_with_info = std::tuple<Point_3, Vector_3, float, unsigned char>;
using Point_map = CGAL::Nth_of_tuple_property_map<0, Point_with_info>;
using Normal_map = CGAL::Nth_of_tuple_property_map<1, Point_with_info>;
using Scan_angle_map = CGAL::Nth_of_tuple_property_map<2, Point_with_info>;
using Scanline_id_map = CGAL::Nth_of_tuple_property_map<3, Point_with_info>;
void dump (const char* filename, const std::vector<Point_with_info>& points)
{
std::ofstream ofile (filename, std::ios::binary);
CGAL::IO::set_binary_mode(ofile);
CGAL::IO::write_PLY
(ofile, points,
CGAL::parameters::point_map (Point_map()).
normal_map (Normal_map()));
}
int main (int argc, char** argv)
{
std::string fname (argc > 1 ? argv[1] : "data/urban.las");
std::vector<Point_with_info> points;
std::cerr << "Reading input file " << fname << std::endl;
std::ifstream ifile (fname, std::ios::binary);
if (!ifile ||
!CGAL::IO::read_LAS_with_properties
(ifile, std::back_inserter (points),
CGAL::IO::make_las_point_reader (Point_map()),
std::make_pair (Scan_angle_map(),
CGAL::IO::LAS_property::Scan_angle()),
std::make_pair (Scanline_id_map(),
CGAL::IO::LAS_property::Scan_direction_flag())))
{
std::cerr << "Can't read " << fname << std::endl;
return EXIT_FAILURE;
}
std::cerr << "Estimating normals" << std::endl;
CGAL::jet_estimate_normals<CGAL::Parallel_if_available_tag>
(points, 12,
CGAL::parameters::point_map (Point_map()).
normal_map (Normal_map()));
std::cerr << "Orienting normals using scan angle and direction flag" << std::endl;
CGAL::scanline_orient_normals
(points,
CGAL::parameters::point_map (Point_map()).
normal_map (Normal_map()).
scan_angle_map (Scan_angle_map()).
scanline_id_map (Scanline_id_map()));
dump("out_angle_and_flag.ply", points);
std::cerr << "Orienting normals using scan direction flag only" << std::endl;
CGAL::scanline_orient_normals
(points,
CGAL::parameters::point_map (Point_map()).
normal_map (Normal_map()).
scanline_id_map (Scanline_id_map()));
dump("out_flag.ply", points);
std::cerr << "Orienting normals using scan angle only" << std::endl;
CGAL::scanline_orient_normals
(points,
CGAL::parameters::point_map (Point_map()).
normal_map (Normal_map()).
scan_angle_map (Scan_angle_map()));
dump("out_angle.ply", points);
std::cerr << "Orienting normals using no additional info" << std::endl;
CGAL::scanline_orient_normals
(points,
CGAL::parameters::point_map (Point_map()).
normal_map (Normal_map()));
dump("out_nothing.ply", points);
return EXIT_SUCCESS;
}
Kernel::Point_3
Kernel::Vector_3
CGAL::scanline_orient_normals
void scanline_orient_normals(PointRange &points, const NamedParameters &np=parameters::default_values())
orients the normals of the range of points by estimating a line of sight and checking its consistency...
Definition: scanline_orient_normals.h:461
CGAL::IO::read_LAS_with_properties
bool read_LAS_with_properties(std::istream &is, PointOutputIterator output, PropertyHandler &&... properties)
CGAL::IO::make_las_point_reader
std::tuple< PointMap, typename Kernel_traits< typename PointMap::value_type >::Kernel::Construct_point_3, LAS_property::X, LAS_property::Y, LAS_property::Z > make_las_point_reader(PointMap point_map)
CGAL::IO::write_PLY
bool write_PLY(std::ostream &out, const PointRange &points, const PolygonRange &polygons, const NamedParameters &np=parameters::default_values())
CGAL::IO::set_binary_mode
Mode set_binary_mode(std::ios &s)
Kernel
CGAL::Nth_of_tuple_property_map
CGAL::Simple_cartesian