CGAL 6.2 - 3D Generalized Barycentric Coordinates

Loading...
Searching...
No Matches
Barycentric_coordinates_3/shape_deformation_3.cpp
#include <CGAL/Exact_predicates_inexact_constructions_kernel.h>
#include <CGAL/Surface_mesh.h>
#include <CGAL/boost/graph/generators.h>
#include <CGAL/boost/graph/IO/polygon_mesh_io.h>
#include <CGAL/Barycentric_coordinates_3.h>
#include <fstream>
using Kernel = CGAL::Exact_predicates_inexact_constructions_kernel;
using Point_3 = Kernel::Point_3;
using Surface_mesh = CGAL::Surface_mesh<Point_3>;
int main(int argc, char** argv) {
const std::string filename = (argc > 1) ? argv[1] : CGAL::data_file_path("meshes/armadillo.off");
Surface_mesh sm;
if(!CGAL::IO::read_polygon_mesh(filename, sm)) {
std::cerr << "Invalid input: " << filename << std::endl;
return 1;
}
Surface_mesh deformed;
deformed = sm;
Surface_mesh quad_cage;
const Point_3 p0( 200, -200, -200), p0_new( 500, -500, -500);
const Point_3 p1( 200, 200, -200), p1_new( 300, 300, -300);
const Point_3 p2(-200, 200, -200), p2_new(-200, 200, -200);
const Point_3 p3(-200, -200, -200), p3_new(-300, -300, -300);
const Point_3 p4(-200, -200, 200), p4_new(-300, -300, 300);
const Point_3 p5( 200, -200, 200), p5_new( 400, -400, 400);
const Point_3 p6( 200, 200, 200), p6_new( 200, 200, 300);
const Point_3 p7(-200, 200, 200), p7_new(-300, 300, 300);
CGAL::make_hexahedron(p0, p1, p2, p3, p4, p5, p6, p7, quad_cage,
CGAL::parameters::do_not_triangulate_faces(false));
CGAL::Barycentric_coordinates::Mean_value_coordinates_3<Surface_mesh> mv(quad_cage);
auto vertex_point_map = get_property_map(CGAL::vertex_point, deformed);
std::vector<double> coords;
std::vector<Point_3> target_cube{p0_new, p1_new, p2_new, p3_new,
p4_new, p5_new, p6_new, p7_new};
for(Surface_mesh::Vertex_index v : vertices(deformed)) {
const Point_3 vertex_val = get(vertex_point_map, v);
coords.clear();
mv(vertex_val, std::back_inserter(coords));
Point_3 p = CGAL::Barycentric_coordinates::apply_barycentric_coordinates_3(target_cube, coords);
put(vertex_point_map, v, p);
}
std::ofstream out_original("armadillo.off");
out_original << sm << std::endl;
std::ofstream out_deformed("deformed_armadillo_mv.off");
out_deformed << deformed << std::endl;
return EXIT_SUCCESS;
}
Barycentric_coordinates_3.h
A convenience header that includes all free functions and classes for 3D barycentric coordinates in c...
CGAL::Barycentric_coordinates::Mean_value_coordinates_3
computes 3D mean value barycentric coordinates with respect to a closed triangle mesh.
Definition: Mean_value_coordinates_3.h:56
CGAL::Exact_predicates_inexact_constructions_kernel
Kernel::Point_3
CGAL::make_hexahedron
boost::graph_traits< Graph >::halfedge_descriptor make_hexahedron(const P &p0, const P &p1, const P &p2, const P &p3, const P &p4, const P &p5, const P &p6, const P &p7, Graph &g, const NamedParameters &np=parameters::default_values())
CGAL::IO::read_polygon_mesh
bool read_polygon_mesh(const std::string &fname, Graph &g, const NamedParameters &np=parameters::default_values())
CGAL::Barycentric_coordinates::apply_barycentric_coordinates_3
boost::property_traits< VertexPointMap >::value_type apply_barycentric_coordinates_3(const TriangleMesh &tmesh, const CoordinateRange &coordinates, VertexPointMap vpm, GeomTraits geom_traits=GeomTraits())
computes a point location from barycentric coordinates with respect to a triangle mesh.
Definition: Barycentric_coordinates_3.h:76
Kernel