CGAL 6.1.1 - Quadtrees, Octrees, and Orthtrees

Loading...
Searching...
No Matches
Orthtree/quadtree_build_from_point_vector.cpp
#include <iostream>
#include <CGAL/Simple_cartesian.h>
#include <CGAL/Quadtree.h>
#include <CGAL/Random.h>
// Type Declarations
using Kernel = CGAL::Simple_cartesian<double>;
using Point_2 = Kernel::Point_2;
using Point_vector = std::vector<Point_2>;
using Quadtree = CGAL::Quadtree<Kernel, Point_vector>;
int main()
{
CGAL::Random r;
Point_vector points_2d;
for (std::size_t i = 0; i < 5; ++ i)
points_2d.emplace_back(r.get_double(-1., 1.),
r.get_double(-1., 1.));
Quadtree quadtree(points_2d);
quadtree.refine(10, 5);
return EXIT_SUCCESS;
}
CGAL::Orthtree
A data structure using an axis-aligned hyperrectangle decomposition of dD space for efficient access ...
Definition: Orthtree.h:117
Kernel::Point_2
Kernel
CGAL::Simple_cartesian