CGAL 6.1.1 - Classification

Loading...
Searching...
No Matches
List of all members | Classes | Public Types
CGAL::Classification::Feature_set Class Reference
Reference Manual » Feature

`#include <CGAL/Classification/Feature_set.h>`

## Definition

sets of features (see `Feature_base`) used as input by classification algorithms.

This class handles both the instantiation, the addition and the deletion of features.

## Public Types
using | const_iterator = unspecified_type
| A random access constant iterator with value type `Feature_handle`.
using | iterator = unspecified_type
| A random access iterator with value type `Feature_handle`.

## Constructor
| Feature_set ()
| creates an empty feature set.

## Modifications
template<typename Feature , typename ... T>
Feature_handle | add (T &&... t)
| instantiates a new feature and adds it to the set.
bool | remove (Feature_handle feature)
| removes a feature.
void | clear ()
| removes all features.

## Parallel Processing
void | begin_parallel_additions ()
| initializes structures to compute features in parallel.
void | end_parallel_additions ()
| waits for the end of parallel feature computation and clears dedicated data structures afterwards.

## Access
const_iterator | begin () const
iterator | begin ()
const_iterator | end () const
iterator | end ()
std::size_t | size () const
| returns how many features are defined.
Feature_handle | operator[] (std::size_t i) const
| returns the \(i^{th}\) feature.

## Member Function Documentation

## ◆ add()

template<typename Feature , typename ... T>

Feature_handle CGAL::Classification::Feature_set::add | ( | T &&... | t | ) |

instantiates a new feature and adds it to the set.

If several calls of `add()` are surrounded by `begin_parallel_additions()` and `end_parallel_additions()`, they are computed in parallel. They are still inserted in the specified order in the feature set (the first call of `add()` creates a feature at index 0, the second at index 1, etc.).

See also
  `begin_parallel_additions()`
  `end_parallel_additions()`

Template Parameters

  Feature | type of the feature, inherited from `Feature_base`.
  T | types of the parameters of the feature's constructor.

Parameters

  t | parameters of the feature's constructor.

Returns
  a handle to the newly added feature.

## ◆ begin_parallel_additions()

void CGAL::Classification::Feature_set::begin_parallel_additions | ( |  | ) |

initializes structures to compute features in parallel.

If the user wants to add features in parallel, this function should be called before making several calls of `add()`. After the calls of `add()`, `end_parallel_additions()` should be called.

Note
  If Intel TBB is not available, this function does nothing.

Warning
  As arguments of `add()` are passed by reference and that new threads are started if `begin_parallel_additions()` is used, it is highly recommended to always call `begin_parallel_additions()`, `add()` and `end_parallel_additions()` within the same scope, to avoid keeping references to temporary objects that might be deleted before the thread has terminated.

See also
  `end_parallel_additions()`

## ◆ end_parallel_additions()

void CGAL::Classification::Feature_set::end_parallel_additions | ( |  | ) |

waits for the end of parallel feature computation and clears dedicated data structures afterwards.

If the user wants to add features in parallel, this function should be called after `begin_parallel_additions()` and several calls of `add()`.

Note
  If Intel TBB is not available, this function does nothing.

See also
  `begin_parallel_additions()`

## ◆ remove()

bool CGAL::Classification::Feature_set::remove | ( | Feature_handle | feature | ) |

removes a feature.

Parameters

  feature | the handle to feature type that must be removed.

Returns
  `true` if the feature was correctly removed, `false` if its handle was not found.