CGAL 6.1.1 - Planar Parameterization of Triangulated Surface Meshes

Loading...
Searching...
No Matches
Classes
Border Parameterization Methods
Reference Manual

##

Border parameterization methods define a set of constraints (a constraint specifies two (u,v) coordinates for each instance of a vertex along the border).

This package implements common border parameterization methods:

- For fixed border methods:
  - the user can select a border parameterization among two common methods: uniform or arc-length parameterizations.
  - one convex shape specified by:
    - one shape among a set of standard ones (circle, square).
- For free border methods: at least two constraints (the pinned vertices).

## Classes
class | CGAL::Surface_mesh_parameterization::Circular_border_parameterizer_3< TriangleMesh_ >
| This is the base class of strategies that parameterize the border of a 3D surface onto a circle. More...
class | CGAL::Surface_mesh_parameterization::Circular_border_uniform_parameterizer_3< TriangleMesh_ >
| This class parameterizes the border of a 3D surface onto a circle in a uniform manner: points are equally spaced. More...
class | CGAL::Surface_mesh_parameterization::Circular_border_arc_length_parameterizer_3< TriangleMesh_ >
| This class parameterizes the border of a 3D surface onto a circle, with an arc-length parameterization: the `(u,v)` values are proportional to the length of border edges. More...
class | CGAL::Surface_mesh_parameterization::Square_border_parameterizer_3< TriangleMesh_ >
| This is the base class of strategies that parameterize the border of a 3D surface onto a square. More...
class | CGAL::Surface_mesh_parameterization::Square_border_uniform_parameterizer_3< TriangleMesh_ >
| This class parameterizes the border of a 3D surface onto a square in a uniform manner: points are equally spaced. More...
class | CGAL::Surface_mesh_parameterization::Square_border_arc_length_parameterizer_3< TriangleMesh_ >
| This class parameterizes the border of a 3D surface onto a square, with an arc-length parameterization: `(u,v)` values are proportional to the length of border edges. More...
class | CGAL::Surface_mesh_parameterization::Two_vertices_parameterizer_3< TriangleMesh_ >
| The class `Two_vertices_parameterizer_3` parameterizes two extreme vertices of a 3D surface. More...