CGAL 6.2 - 3D Surface Mesh Generation

Loading...
Searching...
No Matches
List of all members
CGAL::Surface_mesh_default_criteria_3< Tr > Class Template Reference
Reference Manual » Mesh and Domain Classes

`#include <CGAL/Surface_mesh_default_criteria_3.h>`

## Definition

template<typename Tr>
class CGAL::Surface_mesh_default_criteria_3< Tr >

The class `Surface_mesh_default_criteria_3` implements the most commonly used combination of meshing criteria.

It involves mainly three criteria which are in order:

- a lower bound on the minimum angle in degrees of the surface mesh facets.

- an upper bound on the radius of surface Delaunay balls. A surface Delaunay ball is a ball circumscribing a facet, centered on the surface and empty of vertices. Such a ball exists for each facet of the current surface mesh. Indeed the current surface mesh is the Delaunay triangulation of the current sampling restricted to the surface which is just the set of facets in the three dimensional Delaunay triangulation of the sampling that have a Delaunay surface ball.

- an upper bound on the center-center distances of the surface mesh facets. The center-center distance of a surface mesh facet is the distance between the facet circumcenter and the center of its surface Delaunay ball.

Is model of
  `SurfaceMeshFacetsCriteria_3`

See also
  `make_surface_mesh`

Examples
  Surface_mesher/mesh_a_3d_gray_image.cpp, and Surface_mesher/mesh_an_implicit_function.cpp.

## Types
typedef Tr::FT | FT
| The numerical type.

## Creation
| Surface_mesh_default_criteria_3 (FT angle_bound, FT radius_bound, FT distance_bound)
| Returns a `Surface_mesh_default_criteria_3` with `angle_bound`, `radius_bound`, `distance_bound` as bounds for the minimum facet angle in degrees, the radius of the surface Delaunay balls and the center-center distances respectively.