CGAL 5.6.3 - 2D and 3D Linear Geometry Kernel

Loading...
Searching...
No Matches
List of all members
CGAL::Iso_cuboid_3< Kernel > Class Template Reference
2D and 3D Linear Geometry Kernel Reference » 3D Kernel Objects

`#include <CGAL/Iso_cuboid_3.h>`

## Definition

template<typename Kernel>
class CGAL::Iso_cuboid_3< Kernel >

An object `c` of the data type `Iso_cuboid_3` is a cuboid in the Euclidean space \( \E^3\) with edges parallel to the \( x\), \( y\) and \( z\) axis of the coordinate system.

Although they are represented in a canonical form by only two vertices, namely the lexicographically smallest and largest vertex with respect to Cartesian \( xyz\) coordinates, we provide functions for "accessing" the other vertices as well.

Iso-oriented cuboids and bounding boxes are quite similar. The difference however is that bounding boxes have always double coordinates, whereas the coordinate type of an iso-oriented cuboid is chosen by the user.

Is Model Of:

  `Kernel::IsoCuboid_3`

  `Hashable` if `Kernel` is a cartesian kernel and if `Kernel::FT` is `Hashable`

## Creation
| Iso_cuboid_3 (const Point_3< Kernel > &p, const Point_3< Kernel > &q)
| introduces an iso-oriented cuboid `c` with diagonal opposite vertices `p` and `q`.
| Iso_cuboid_3 (const Point_3< Kernel > &p, const Point_3< Kernel > &q, int)
| introduces an iso-oriented cuboid `c` with diagonal opposite vertices `p` and `q`.
| Iso_cuboid_3 (const Point_3< Kernel > &left, const Point_3< Kernel > &right, const Point_3< Kernel > &bottom, const Point_3< Kernel > &top, const Point_3< Kernel > &far, const Point_3< Kernel > &close)
| introduces an iso-oriented cuboid `c` whose minimal \( x\) coordinate is the one of `left`, the maximal \( x\) coordinate is the one of `right`, the minimal \( y\) coordinate is the one of `bottom`, the maximal \( y\) coordinate is the one of `top`, the minimal \( z\) coordinate is the one of `far`, the maximal \( z\) coordinate is the one of `close`.
| Iso_cuboid_3 (const Kernel::RT &min_hx, const Kernel::RT &min_hy, const Kernel::RT &min_hz, const Kernel::RT &max_hx, const Kernel::RT &max_hy, const Kernel::RT &max_hz, const Kernel::RT &hw=RT(1))
| introduces an iso-oriented cuboid `c` with diagonal opposite vertices (`min_hx/hw`, `min_hy/hw`, `min_hz/hw`) and (`max_hx/hw`, `max_hy/hw`, `max_hz/hw`).
| Iso_cuboid_3 (const Bbox_3 &bbox)
| If `Kernel::RT` is constructible from double, introduces an iso-oriented cuboid from `bbox`.

## Operations
bool | operator== (const Iso_cuboid_3< Kernel > &c2) const
| Test for equality: two iso-oriented cuboid are equal, iff their lower left and their upper right vertices are equal.
bool | operator!= (const Iso_cuboid_3< Kernel > &c2) const
| Test for inequality.
Point_3< Kernel > | vertex (int i) const
| returns the i'th vertex modulo 8 of `c`.
Point_3< Kernel > | operator[] (int i) const
| returns `vertex(i)`, as indicated in the figure below:
Point_3< Kernel > | min () const
| returns the smallest vertex of `c` (= `vertex(0)`).
Point_3< Kernel > | max () const
| returns the largest vertex of `c` (= `vertex(7)`).
Kernel::FT | xmin () const
| returns smallest Cartesian \( x\)-coordinate in `c`.
Kernel::FT | ymin () const
| returns smallest Cartesian \( y\)-coordinate in `c`.
Kernel::FT | zmin () const
| returns smallest Cartesian \( z\)-coordinate in `c`.
Kernel::FT | xmax () const
| returns largest Cartesian \( x\)-coordinate in `c`.
Kernel::FT | ymax () const
| returns largest Cartesian \( y\)-coordinate in `c`.
Kernel::FT | zmax () const
| returns largest Cartesian \( z\)-coordinate in `c`.
Kernel::FT | min_coord (int i) const
| returns `i`-th Cartesian coordinate of the smallest vertex of `c`.
Kernel::FT | max_coord (int i) const
| returns `i`-th Cartesian coordinate of the largest vertex of `c`.

## Predicates
bool | is_degenerate () const
| `c` is degenerate, if all vertices are coplanar.
Bounded_side | bounded_side (const Point_3< Kernel > &p) const
| returns either ON_UNBOUNDED_SIDE, ON_BOUNDED_SIDE, or the constant ON_BOUNDARY, depending on where point `p` is.
bool | has_on_boundary (const Point_3< Kernel > &p) const
bool | has_on_bounded_side (const Point_3< Kernel > &p) const
bool | has_on_unbounded_side (const Point_3< Kernel > &p) const

## Miscellaneous
Kernel::FT | volume () const
| returns the volume of `c`.
Bbox_3 | bbox () const
| returns a bounding box containing `c`.
Iso_cuboid_3< Kernel > | transform (const Aff_transformation_3< Kernel > &t) const
| returns the iso-oriented cuboid obtained by applying `t` on the smallest and the largest of `c`.

## Constructor & Destructor Documentation

## ◆ Iso_cuboid_3() [1/3]

template<typename Kernel >

CGAL::Iso_cuboid_3< Kernel >::Iso_cuboid_3 | ( | const Point_3< Kernel > & | p,
|  | const Point_3< Kernel > & | q
| ) |  |

introduces an iso-oriented cuboid `c` with diagonal opposite vertices `p` and `q`.

Note that the object is brought in the canonical form.

## ◆ Iso_cuboid_3() [2/3]

template<typename Kernel >

CGAL::Iso_cuboid_3< Kernel >::Iso_cuboid_3 | ( | const Point_3< Kernel > & | p,
|  | const Point_3< Kernel > & | q,
|  | int |
| ) |  |

introduces an iso-oriented cuboid `c` with diagonal opposite vertices `p` and `q`.

The `int` argument value is only used to distinguish the two overloaded functions.

Precondition
  `p.x()<=q.x()`, `p.y()<=q.y()` and `p.z()<=q.z()`.

## ◆ Iso_cuboid_3() [3/3]

template<typename Kernel >

CGAL::Iso_cuboid_3< Kernel >::Iso_cuboid_3 | ( | const Kernel::RT & | min_hx,
|  | const Kernel::RT & | min_hy,
|  | const Kernel::RT & | min_hz,
|  | const Kernel::RT & | max_hx,
|  | const Kernel::RT & | max_hy,
|  | const Kernel::RT & | max_hz,
|  | const Kernel::RT & | hw = `RT(1)`
| ) |  |

introduces an iso-oriented cuboid `c` with diagonal opposite vertices (`min_hx/hw`, `min_hy/hw`, `min_hz/hw`) and (`max_hx/hw`, `max_hy/hw`, `max_hz/hw`).

Precondition
  `hw != 0`.

## Member Function Documentation

## ◆ max_coord()

template<typename Kernel >

Kernel::FT CGAL::Iso_cuboid_3< Kernel >::max_coord | ( | int | i | ) | const

returns `i`-th Cartesian coordinate of the largest vertex of `c`.

Precondition
  `0 <= i <= 2`.

## ◆ min_coord()

template<typename Kernel >

Kernel::FT CGAL::Iso_cuboid_3< Kernel >::min_coord | ( | int | i | ) | const

returns `i`-th Cartesian coordinate of the smallest vertex of `c`.

Precondition
  `0 <= i <= 2`.

## ◆ operator[]()

template<typename Kernel >

Point_3< Kernel > CGAL::Iso_cuboid_3< Kernel >::operator[] | ( | int | i | ) | const

returns `vertex(i)`, as indicated in the figure below:

## ◆ transform()

template<typename Kernel >

Iso_cuboid_3< Kernel > CGAL::Iso_cuboid_3< Kernel >::transform | ( | const Aff_transformation_3< Kernel > & | t | ) | const

returns the iso-oriented cuboid obtained by applying `t` on the smallest and the largest of `c`.

Precondition
  The angle at a rotation must be a multiple of \( \pi/2\), otherwise the resulting cuboid does not have the same size. Note that rotating about an arbitrary angle can even result in a degenerate iso-oriented cuboid.

## ◆ vertex()

template<typename Kernel >

Point_3< Kernel > CGAL::Iso_cuboid_3< Kernel >::vertex | ( | int | i | ) | const

returns the i'th vertex modulo 8 of `c`.

starting with the lower left vertex.